1 CCR 301-25

6.4 Effective January 1, 2025, pursuant to Section 8 of these rules, vehicles with a capacity of more than 12 passengers that do not meet the definition of a Type A School Bus or a Type A Multifunction Bus, or meet the Colorado Rack and Load, Kentucky Pole Test, and FMVSS School Bus Safety Standards, as required, are prohibited from transporting students for any reason.